<html><head><meta name="color-scheme" content="light dark"></head><body><pre style="word-wrap: break-word; white-space: pre-wrap;">;; PSPad code template for Code V interferogram
;; Author: Francois Riguet
;; Update: 27/06/2006
;; Update: 28/10/2013 =&gt; added WVL 1 into the header generated by @PGM_TO_INT
;;                       to enable importing into Gwyddion  
[Macro definition]
%00title%=@E, Title,,Code V interferogram
%nodata%=@E, No data value,,32767
%numterms%=@E, Number of terms,,9
%routinename%=@E, Routine name,,,,'
%datafile%=@E, External data file,,,,'
%wavelength%=@E, Wavelength in microns,,0.6328
%scale%=@E, Scale size,,32760
%xyratio%=@E, X/Y ratio,,1
%x%=@E, X number of points,,10
%y%=@E, Y nbr of points or R,,10
%01datatype%=@C Data format type,,GRD,GRD;ZRN;ZFR;UDI,
%02val1%=@E, X GRD / Nterms ZRN/ZFR/UDI, 
%03val2%=@E, Y or R for GRD,
%04filetype%=@C File type,,FIL,BIR;CAO;FIL;SUR;THV;WFR,
%05wvl%=@K, Wavelength ?,WVL,
%06val3%=@E, Wvl in µm (0.6328),,,
%07nnb%=@K, Nearest neighbor ?,NNB,
%08val4%=@E, Scale size (&lt;=&gt;1 for FIL),,32760,
%09nda%=@K, No data,NDA,
%10val5%=@E, No data value (32767),,
%11xsc%=@K, X/Y ratio ?,XSC,
%12val6%=@E, X/Y ratio,
%13umr%=@K, Subroutine ?, 
%14val7%=@E, Subroutine (for UDI),,,,'
%15umf%=@K, External data file ?,
%16val8%=@E, Ext. data file (for UDI),,,,'
%01Xpixels%=@E Number of X pixels ?,,
%02Ypixels%=@E Number of Y pixels ?,,
%03ssz%=@E Normalizing value,,255
[&amp;TEMPLATE | Create interferogram header ]
%00title%
%01datatype% %02val1% %03val2% %04filetype% %05wvl% %06val3% %07nnb% SSZ %08val4% %09nda% %10val5% %11xsc% %12val6% %13umr% %14val7% %15umf% %16val8% 
|
[@PGM TO INT | Change PGM header to INT format ]
%00title%
GRD %01Xpixels% %02Ypixels% FIL WVL 1 SSZ %03ssz% %11xsc% %12val6%
|
[COMMENT | Insert comment ]
! |
[BIR | Birefringence magnitude file ]
BIR |
[CAO | Crystal axis orientation file ]
CAO |
[FIL | Intensity apodization file ]
FIL |
[GRD | Grid data ]
GRD %x% %y% |
[NDA | No data value ]
NDA %nodata% |
[NNB | Nearest neighbor ]
NNB |
[R | Radial grid data ]
R |
[SSZ | Scale size ]
SSZ %scale% |
[SUR | Surface interferogram ]
SUR |
[THV | Coating thickness variation file ]
THV |
[UDI | User-defined data ]
UDI %numterms% |
[UMF | User-defined external data file ]
UMF %datafile% |
[UMR | User-defined subroutine / macro ]
UMR %routinename% |
[WFR | Wavefront interferogram ]
WFR |
[WVL | Wavelength ]
WVL %wavelength% |
[XSC | X scale ]
XSC %xyratio% |
[ZFR | Fringe Zernike data ]
ZFR %numterms% |
[ZRN | Zernike data ]
ZRN %numterms% |

</pre></body></html>